,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Sound pressure level_Heating(Med)##OTHER##,Sound pressure level_Heating(Low)##OTHER##,Sound pressure level_Heating(High)##OTHER##,Sound pressure level_Cooling(Med)##OTHER##,Sound pressure level_Cooling(Low)##OTHER##,Sound pressure level_Cooling(High)##OTHER##,Sound power level_Heating(High)##OTHER##,Sound power level_Cooling(High)##OTHER##,SEER_Cooling##OTHER##,SCOP_Heating (Average)##OTHER##,Rated Input power_Heating##ELECTRICAL_POWER##KILOWATTS,Rated Input power_Cooling##ELECTRICAL_POWER##KILOWATTS,Power Connection Offset Right##LENGTH##MILLIMETERS,Phase##OTHER##,Pdesign_Heating (Average)##OTHER##,Pdesign_Cooling##OTHER##,Operation range_Heating##OTHER##,Operation range_Cooling##OTHER##,Number of Poles##OTHER##,Model##OTHER##,Width##LENGTH##MILLIMETERS,URL##OTHER##,Refrigerant Used##OTHER##,Rated Heating Capacity##HVAC_HEATING_LOAD##KILOWATTS,Rated Cooling Capacity##HVAC_COOLING_LOAD##KILOWATTS,Product Weight##OTHER##,Product Documentation Link##OTHER##,Power Connection Offset Bottom##LENGTH##MILLIMETERS,Manufacturer##OTHER##,Liquid Connection Radius##LENGTH##MILLIMETERS,Liquid Connection Offset Right##LENGTH##MILLIMETERS,Liquid Connection Offset Bottom##LENGTH##MILLIMETERS,Liquid Connection Diameter##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,Gas Connection Diameter##LENGTH##MILLIMETERS,Gas Connection  Radius##LENGTH##MILLIMETERS,Gas Connection  Offset Right##LENGTH##MILLIMETERS,Gas Connection  Offset Bottom##LENGTH##MILLIMETERS,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Equipment Material##OTHER##,Energy efficiency class_Heating (Average)##OTHER##,Energy efficiency class_Cooling##OTHER##,EER_Cooling##OTHER##,Depth##LENGTH##MILLIMETERS,Copyright ©##OTHER##,Connection Cutout Radius##LENGTH##MILLIMETERS,Connection Cutout Offset Right##LENGTH##MILLIMETERS,Connection Cutout Offset Left##LENGTH##MILLIMETERS,Connection Cutout Diameter##LENGTH##MILLIMETERS,Condensate Drain Connection Radius##LENGTH##MILLIMETERS,Condensate Drain Connection Offset Right##LENGTH##MILLIMETERS,Condensate Drain Connection Offset Bottom##LENGTH##MILLIMETERS,Condensate Drain Connection Diameter##OTHER##,Clearance Offset Top##LENGTH##MILLIMETERS,Clearance Offset Right##LENGTH##MILLIMETERS,Clearance Offset Left##LENGTH##MILLIMETERS,Clearance Offset Front##LENGTH##MILLIMETERS,Clearance Offset Bottom##LENGTH##MILLIMETERS,Clearance Offset Back##LENGTH##MILLIMETERS,COP_Heating##OTHER##,Available voltage range##OTHER##,Annual energy consumption_QHE (Average)##OTHER##,Annual energy consumption_QCE##OTHER##,Airflow rate_Heating(Med)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Airflow rate_Heating(Low)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Airflow rate_Heating(High)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Airflow rate_Cooling(Med)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Airflow rate_Cooling(Low)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR,Airflow rate_Cooling(High)##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR
ASYG18KLCA,230,45 dB(A),41 dB(A),50 dB(A),44 dB(A),40 dB(A),47 dB(A),65 dB(A),60 dB(A),7.20 kWh/kWh,4.30 kWh/kWh,1.8,1.685,52,1,4.8 kW(-10 C.degree),5.2 kW(35 C.degree),16 to 30 C.degree,18 to 32 C.degree,2,ASYG18KLCA,790,http://www.fujitsu-general.com/index.html,R32,6.3,5.2,9.5 kg,,45,FUJITSU GENERAL LIMITED,3.175,62,30,6.35,293,9.52,4.76,57,65,50.000000000000,Plastic - Fujitsu General - White,A+,A++,3.09 kW/kW,249,Copyright©2017 Fujitsu General Limited. All rights reserved.,32.5,70,63,65,8.35,82,50,"φ 13.8 (I.D.), φ 15.8 to φ 16.7 (O.D.)",65,48,52,"1,500","1,800",0,3.50 kW/kW,198 to 264V,1563 kWh/a,253 kWh/a,810,700,995,780,665,865
ASYG24KLCA,230,45 dB(A),41 dB(A),52 dB(A),45 dB(A),38 dB(A),51 dB(A),65 dB(A),64 dB(A),7.10 kWh/kWh,4.00 kWh/kWh,2.225,2.42,52,1,7.1 kW(-10 C.degree),7.1 kW(35 C.degree),16 to 30 C.degree,18 to 32 C.degree,2,ASYG24KLCA,790,http://www.fujitsu-general.com/index.html,R32,8,7.1,10 kg,,45,FUJITSU GENERAL LIMITED,3.175,62,30,6.35,293,12.7,6.35,57,65,50.000000000000,Plastic - Fujitsu General - White,A+,A++,2.93 kW/kW,249,Copyright©2017 Fujitsu General Limited. All rights reserved.,32.5,70,63,65,8.35,82,50,"φ 13.8 (I.D.), φ 15.8 to φ 16.7 (O.D.)",65,48,52,"1,500","1,800",0,3.60 kW/kW,198 to 264V,2485 kWh/a,350 kWh/a,800,680,"1,040",880,685,"1,040"
